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Escambia County Weekly Sampling Report  
September 3, 2010

The Florida Department of Environmental Protection is collecting and analyzing water, sediment, and oil samples from Florida’s coastal waters in response to the Deepwater Horizon oil spill.  These samples are being collected for a variety of purposes.  There is a delay from when the samples are collected to when the results are reported due to the time that it takes to deliver the samples to the lab and then analyze the samples.  We are striving for a four day turnaround time.  Results will be reported on a weekly basis (on Fridays).  
New Information Week of August 30th – September 3rd: 
· Week of August 30th through September 3rd, 2010, water quality samples were collected on Monday and Thursday.   There are plans to sample twice a week in all 7 counties.  Sampling in Franklin and Gulf County took place on Tuesday.  Water samples will be analyzed for PAH’s.  
·  Note: For new water quality result information please see information highlighted in yellow below.  
The following sampling was performed in Escambia County:
· Routine water sampling was conducted on Monday and Thursday this week.
· Results reported below for 8/26/10 sampling events and results of 6/24/10 dispersant analysis are also listed.
Post Impact Sampling (Reporting results from August 26th through September 3rd, 2010):

	Date Sampled
	Sampling Information
	Results

	PENSACOLA BEACH @ FT.  PICKENS

	8/26/2010 10:15
	Water Sample
	No petroleum-related contaminants were found.

	8/30/2010  9:55
	Water Sample
	No petroleum-related contaminants were found.

	PERDIDO KEY-JOHNSON BEACH

	8/26/2010 9:20
	Water sample
	No petroleum-related contaminants were found.

	8/30/2010  8:55
	Water sample
	No petroleum-related contaminants were found.

	6/24/2010  6:15
	Collected for Dispersant Analysis
	No Dioctylsulfosuccinate-Na** was found.

	PENSACOLA BEACH EAST OF PIER

	8/26/2010 10:35
	Water Sample
	No petroleum-related contaminants were found.

	8/30/2010 10:20
	Water Sample
	No petroleum-related contaminants were found.

	NAVARRE PARK*

	8/26/2010 11:10
	Water sample
	No petroleum-related contaminants were found.

	8/30/2010  11:05
	Water sample
	No petroleum-related contaminants were found.

	Pensacola Beach

	6/23/2010  4:35
	Collected for Dispersant Analysis
	No Dioctylsulfosuccinate-Na** was found.

	6/23/2010  7:00
	Collected for Dispersant Analysis
	No Dioctylsulfosuccinate-Na** was found.

	Gulf Island Nat’l Seashore

	6/24/2010  1:45
	Collected for Dispersant Analysis
	No Dioctylsulfosuccinate-Na** was found.


*by lat/longs, area sampled in Escambia County
Table Explanation:
· Water sample – indicates a water sample that was taken, no oil was visible in the water when the sample was taken.

· Sand sample – indicates a sand sample that was taken to evaluate any potential petroleum contamination.  

· “10 cm from visible tar ball”, “1 meter from visible tar ball”, “near oil sheen and/or tar balls” or “Near mousse”– These are types of proximity sampling that means samples were collected at known distances from oil material.  This sampling is performed when the oil in the water is sparse enough that a bather might reasonably expect to swim in the water without coming into contact with the oil.  

· Collected for dispersant analysis – These samples are collected to attempt to detect dispersant.  The first priority is to collect the sample in proximity to oil when oil is present.  When oil is not present the second priority is to sample in locations were oil was previously present.  The third priority is to collect the sample where no oil contamination is, or ever was, present. * * Of the Corexit dispersant products that were used during the Deepwater Horizon Oil Spill, Dioctylsulfosuccinate-Na is the component that is most likely to persist in the water.
For additional information, please refer to the DEP Deepwater Horizon website at http://www.dep.state.fl.us/deepwaterhorizon/default.htm 
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