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Santa Rosa County Daily Sampling Report
July 8, 2010
The Florida Department of Environmental Protection is collecting and analyzing water, sediment, and oil samples from Florida’s coastal waters in response to the Deepwater Horizon oil spill.  These samples are being collected for a variety of purposes.  There is a delay from when the samples are collected to when the results are reported due to the time that it takes to deliver the samples to the lab and then analyze the samples.  We are striving for a four day turnaround time.  Results will be reported on a daily basis.  
New information for July 8, 2010: 

· July 3, 4, 5, 2010 – New sample results available. 

· Proposed – Week of July 5-8.  2 water samples per day are planned for Thursday, July 8.  If oil product is seen in the water, we will sample in proximity to it.  Sampling is proposed to continue next week at 2 water samples per day on Sunday, Tuesday and Thursday.
· Note: Waiting for lat/longs for the Santa Rosa #1 and #2 sites. 
· The following sampling has been performed in Santa Rosa County:

· Tuesday, July 6, 2010: Santa Rosa #1; No oil in water, beach is clear. Rainy and very windy conditions. Santa Rosa #2; Water very churned up, took sample, water appeared “dark”. Conditions very rough surf. 

	Date Sampled
	Sampling Information
	Results

	NAVARRE BEACH

	6/22/10
	Water sample
	No petroleum contaminants were found

	6/22/10 
	Collected for dispersant analysis
	Results are due in 3-4 weeks

	6/28/10
	Water sample
	No petroleum contaminants were found

	NAVARRE BEACH FISHING PIER

	6/25/10
	Water sample
	No petroleum contaminants were found

	6/29/10
	Water sample
	No petroleum contaminants were found

	7/2/10
	Water sample
	No petroleum contaminants were found

	7/3/2010
	Water sample
	No petroleum constituents were found

	7/4/2010
	Water sample
	No petroleum constituents were found

	7/5/2010
	Water sample
	No petroleum constituents were found

	NAVARRE BEACH WEST

	6/29/10
	Water sample
	No petroleum contaminants were found

	7/2/10
	Water sample
	No petroleum contaminants were found

	7/3/2010
	Water sample
	No petroleum constituents were found

	7/4/2010
	Water sample
	No petroleum constituents were found

	7/5/2010
	Water sample
	No petroleum constituents were found

	NAVARRE BEACH PARK

	6/29/10
	Water sample
	No petroleum contaminants were found


Table Explanation:

· Water sample – indicates a water sample that was taken, no oil was visible in the water when the sample was taken.

· Sand sample – indicates a sand sample that was taken to evaluate any potential petroleum contamination.  
· 10 cm from visible tar ball/1 meter from visible tar ball – These are types of proximity sampling that means samples were collected at known distances from oil.  This sampling is performed when the oil in the water is sparse enough that a bather might reasonably expect to swim in the water without coming into contact with the oil.  

· Collected for dispersant analysis – These samples are collected to attempt to detect dispersant.  The first priority is to collect the sample in proximity to oil when oil is present.  When oil is not present the second priority is to sample in locations were oil was previously present, the third priority is to collect the sample where no oil contamination is, or ever was, present.  

None of the results listed above suggest that recreational activities should be restricted; however, the movement of oil product is unpredictable and conditions at a given location can change rapidly. The public should be advised not to go in the water with visible petroleum products.
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