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Santa Rosa County Daily Sampling Report
July 13, 2010
The Florida Department of Environmental Protection is collecting and analyzing water, sediment, and oil samples from Florida’s coastal waters in response to the Deepwater Horizon oil spill.  These samples are being collected for a variety of purposes.  There is a delay from when the samples are collected to when the results are reported due to the time that it takes to deliver the samples to the lab and then analyze the samples.  We are striving for a four day turnaround time.  Results will be reported on a daily basis.  
New information for July 13, 2010: 

· Proposed – Week of July 9-15.  2 water samples per day are planned for Sunday, Tuesday and Thursday.  If oil product is seen in the water, we will sample in proximity to it.  
· The following sampling has been performed in Santa Rosa County:

· Tuesday, July 13; two water quality samples collected. Field conditions not yet reported.  
	Date Sampled
	Sampling Information
	Results

	NAVARRE BEACH

	
	
	

	NAVARRE BEACH FISHING PIER

	7/8/10
	Water sample
	A small amount of a gas/diesel contaminant (naphthalene) was detected. This is not believed to be associated with the Deepwater Horizon oil spill.

	NAVARRE BEACH WEST

	
	
	

	NAVARRE BEACH PARK

	
	
	


Table Explanation:

· Water sample – indicates a water sample that was taken, no oil was visible in the water when the sample was taken.

· Sand sample – indicates a sand sample that was taken to evaluate any potential petroleum contamination.  
· 10 cm from visible tar ball/1 meter from visible tar ball – These are types of proximity sampling that means samples were collected at known distances from oil.  This sampling is performed when the oil in the water is sparse enough that a bather might reasonably expect to swim in the water without coming into contact with the oil.  

· Collected for dispersant analysis – These samples are collected to attempt to detect dispersant.  The first priority is to collect the sample in proximity to oil when oil is present.  When oil is not present the second priority is to sample in locations were oil was previously present, the third priority is to collect the sample where no oil contamination is, or ever was, present.  

For additional information, please refer to the DEP Deepwater Horizon website at http://www.dep.state.fl.us/deepwaterhorizon/default.htm
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