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Walton County Daily Report
August 12, 2010
The Florida Department of Environmental Protection is collecting and analyzing water, sediment, and oil samples from Florida’s coastal waters in response to the Deepwater Horizon oil spill.  These samples are being collected for a variety of purposes.  There is a delay from when the samples are collected to when the results are reported due to the time that it takes to deliver the samples to the lab and then analyze the samples.  We are striving for a four day turnaround time.  Results will be reported on a daily basis.  
New information for August 12, 2010: 
Week of August 6-12
· Two routine water sample results to report.  No samples were collected today.  
· Proposed routine sampling for this week:  Monday and Thursday (collecting 2 samples each day).
· Note:  New water quality result information highlighted in yellow below. If oil product is seen in the water, we will sample in proximity to it.  If no oil is seen we will likely sample in locations such as Miramar Beach, Blue Mountain Beach, and Grayton Beach.   
· Note: For new water quality results information please see the rows highlighted in yellow below.
The following sampling has been performed in Walton County:

	Date Sampled
	Sampling Information
	Results

	

	BLUE MOUNTAIN BEACH

	6/22/2010  
	Water sample analyzed for dispersant
	No Dioctylsulfosuccinate-Na* was found.

	DEER LAKE STATE PARK

	
	
	

	ED WALLINE PARK

	
	
	

	 GRAYTON BEACH STATE PARK

	8/5/2010
	Water Sample
	No petroleum-related contaminants were found.

	8/9/2010
	Water Sample
	No petroleum-related contaminants were found.

	
	
	

	MIRAMAR BEACH

	6/22/2010  
	Water sample analyzed for dispersant
	No Dioctylsulfosuccinate-Na* was found.

	8/5/2010
	Water Sample
	No petroleum-related contaminants were found.

	8/9/2010
	Water Sample
	No petroleum-related contaminants were found.

	SEAGROVE BEACH

	
	
	

	SEASIDE @ CR 395

	 
	
	

	SEASIDE @ WESTERN LAKE DR

	6/22/2010
	Water sample analyzed for dispersant
	No Dioctylsulfosuccinate-Na* was found.

	
	
	

	SOUTH WALTON BEACH – DUNE ALLEN
	
	

	
	
	

	
	
	

	ALLEN REGIONAL BEACH ACCESS 
	
	

	
	
	

	SEASIDE BEACH  
	
	

	
	
	


* Of the Corexit dispersant products that were used during the Deepwater Horizon Oil Spill, Dioctylsulfosuccinate-Na is the component that is most likely to persist in the water
Table Explanation:

· Water sample – indicates a water sample that was taken, no oil was visible in the water when the sample was taken.

· Sand sample – indicates a sand sample that was taken to evaluate any potential petroleum contamination.  
· 10 cm from visible tar ball/1 meter from visible tar ball – These are types of proximity sampling that means samples were collected at known distances from oil.  This sampling is performed when the oil in the water is sparse enough that a bather might reasonably expect to swim in the water without coming into contact with the oil.  

· Collected for dispersant analysis – These samples are collected to attempt to detect dispersant in the water where no oil contamination has been observed.  

For additional information, please refer to the DEP Deepwater Horizon website at http://www.dep.state.fl.us/deepwaterhorizon/default.htm
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