[image: image1.jpg]EERPWATER

ORIZON

coesls)

ESPONSE ™




[image: image1.jpg]

Walton County Report
Week of September 6 - September 10, 2010
The Florida Department of Environmental Protection is collecting and analyzing water, sediment, and oil samples from Florida’s coastal waters in response to the Deepwater Horizon oil spill.  These samples are being collected for a variety of purposes.  There is a delay from when the samples are collected to when the results are reported due to the time that it takes to deliver the samples to the lab and then analyze the samples.  We are striving for a four day turnaround time.  
New information: 
Week of September 6 - September 10
· On Tuesday (9/7) and Thursday (9/9) two routine water quality samples were collected.
· Lab results from samples collected on 9/2 and 9/7 have been included.
· Proposed Sampling:  This is the last week that water quality samples will be collected.  Beginning next week, no routine water quality sampling will be conducted.
· Note:  If oil product is seen in the water, we will sample in proximity to it.
The following sampling has been performed in Walton County:

	Date Sampled
	Sampling Information
	Results

	

	 GRAYTON BEACH STATE PARK

	9/2/2010
	Water sample collected in proximity to a tarball
	No petroleum-related contaminants were found.

	9/7/2010
	Water sample (1)
	No petroleum-related contaminants were found.

	9/7/2010
	Water sample (2)
	No petroleum-related contaminants were found.

	MIRAMAR BEACH

	9/2/2010
	Water sample
	No petroleum-related contaminants were found.

	9/7/2010
	Water sample
	No petroleum-related contaminants were found.


Table Explanation:
· Water sample – indicates a water sample that was taken, no oil was visible in the water when the sample was taken.

· Sand sample – indicates a sand sample that was taken to evaluate any potential petroleum contamination.  
· 10 cm from visible tar ball/1 meter from visible tar ball – These are types of proximity sampling that means samples were collected at known distances from oil.  This sampling is performed when the oil in the water is sparse enough that a bather might reasonably expect to swim in the water without coming into contact with the oil.  

· Collected for dispersant analysis – These samples are collected to attempt to detect dispersant in the water where no oil contamination has been observed.  

For additional information, please refer to the DEP Deepwater Horizon website at http://www.dep.state.fl.us/deepwaterhorizon/default.htm
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