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Canal St WWTP FLA105066 Turnpike WWTP FLA105147

Permitted Capacity: Permitted Capacity:

3.5MGD 4.5MGD

Permitted TN and TP effluent limits: Permitted TN and TP effluent limits:

Report MAX Report MAX

Annual TN and TP (flow and concentrations) past 5 years Annual TN and TP (flow and concentrations) past 5 years

2023 R001 TN 11.3mg/L 2023 R001 TN 8.1mg/L

AADF 0.2 MGD TP 1.6mg/L AADF 0.6 MGD TP 4.5mg/L

R002 TN 9.2mg/L R002 TN 8.1mg/L

AADF 1.9 MGD TP 1.9mg/L AADF 1.9 MGD TP 4.5mg/L

2022 R001 TN 7.8mg/L 2022 R001 TN 8mg/L

AADF 0.4 MGD TP 1mg/L AADF 1.4 MGD TP 6.3mg/L

R002 TN 8.4mg/L R002 TN 8mg/L

AADF 2.1 MGD TP 2mg/L AADF 1.3 MGD TP 6.3mg/L

2021 R001 TN 3.5mg/L 2021 R001 TN 10.5mg/L

AADF 0.08 MGD TP 1.1mg/L AADF 1.3 MGD TP 1.7mg/L

R002 TN 3.8mg/L R002 TN 10.5mg/L

AADF 2.6 MGD TP 2.4mg/L AADF 0.9 MGD TP 1.7mg/L

2020 R001 TN 0.3mg/L 2020 R001 TN 7.4mg/L

AADF 0.02 MGD TP 0.3mg/L AADF 0.6 MGD TP 2.1mg/L

R002 TN 2.4mg/L R002 TN 7.4mg/L

AADF 2.3 MGD TP 2.6mg/L AADF 1.2 MGD TP 2.1mg/L

2019 R001 TN 0mg/L 2019 R001 TN 13.8mg/L

AADF 0 TP 0mg/L AADF 0.9 MGD TP 1.1mg/L

R002 TN 1.6mg/L R002 TN 13.8mg/L

AADF 2.2 MGD TP 2.3mg/L AADF 0.5 MGD TP 1.1mg/L


