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Caloosahatchee Creeks Water Quality Monitoring
Full Project Name: Caloosahatchee Creeks Water Quality Monitoring
Start Date: 1/2011
Projected End Date:  TBD
Sample Days:  Once monthly, usually takes around 4 hours
Cooperators: Gary Snorek 
Project Lead: Gary Snorek 
File Location: \\publicfiles\PUBFDS\DEAR\WQAPmonitoring\SpecialProjects\20XX\21FLFTM\Caloosahatchee Creeks Sampling
Final Data Repository: WIN
We sample 3 strategically picked tributaries of the Caloosahatchee River.  Orange River, Telegraph Creek, And Hancock Creek are all sampled for BOD-UNIN, CHLSUITE-W, ALKALINITY, W-COLOR, W-DOC, W-F, W-NH3, W-NO2NO3, W-PO4-F, W-S-A-TP, W-TKN, W-TOC, and W-TSS
Sample locations:
	WBID

	WATERBODY NAME

	STATION NAME

	STATION #

	RECEIVING WB

	COUNTY

	LAT

	LONG


	
	
	
	
	
	
	
	

	3240K
	Orange River
	Orange River at Boat Ramp
	G3SD0128
	Caloosahatchee
	Lee
	26.69287
	-81.76737

	3236A
	Telegraph Creek
	Telegraph Creek Sonde @ USGS Sonde Station
	G3SD0129
	Caloosahatchee
	Lee
	26.730561
	-81.701668

	3240E
	Hancock Creek
	Hancock Creek @ Hancock Bridge Parkway
	[bookmark: _GoBack]G3SD0130
	Caloosahatchee
	Lee
	26.6667364
	-81.896507



Notes: Water quality of Hancock Creek, Telegraph Creek, and Orange River is monitored monthly at one site each to support the Caloosahatchee River Basin Management Action Plan.  The suites we collect include: 
· [bookmark: _Hlk13663499]BOD-UNIN
· CHLSUITE-W
· ALKALINITY
· W-COLOR
· W-DOC
· W-F
· W-NH3
· W-NO2NO3
· W-PO4-F 
· W-S-A-TP
· W-TKN
· W-TOC
· W-TSS

