EXAXOL

manufacturers of laboratory solutions/standards since 1988 
CERTIFICATE OF ANALYSIS
Product: Conductivity Standard, 1,000 (-mhos  (C1065-1000)
Lot: 161216A

Expires: (1 yr) 12/2017
Assay (ppm, M, N, %, etc)
Actual: 1,000 

Contains:   Potassium chloride, water: both ACS

Other results: 1000  (-mhos  @  25° C


TDS= 525.0 ppm KCl
Made in accordance with written standard Good Laboratory Practice Procedures. Volumetric glassware used is strictly Class A per ASTM E288 requirements, maintained in accordance with ASTM E 542.  Analytical balance(s) calibrated periodically using certified Class S NIST weights, and documented.  Thermometers used are NIST calibrated.  Standardized products prepared according to Master Lab Record book, with lot #, batch size, customer , and testing results.  

STORAGE: ambient (15 degC-30 degC) 

Standards used:
NIST: Potassium Chloride KCl 3193
Exaxol:

Joseph E Papa, Sr. Chemist     

EXAXOL CHEMICAL CORP, 14325 60th St N, Clearwater, FL 33760
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