Hazardous Waste ADaPT Information

Automated Data Processing Tool (ADaPT) software was developed for the automated evaluation of environmental quality data. ADaPT runs under Microsoft Access and is a tool that laboratories, consultants, solid and hazardous waste facility permittees and Department staff can all use to evaluate groundwater data. ADaPT performs the following functions:
· an error check for correctness and completeness of the data;
· checks blank contamination rules and accuracy and precision criteria for each method and sample matrix;
· performs a data review that measures integrity of sample results against associated laboratory quality control, holding times, and method detection limits;
· checks the results for compliance against user selectable criteria and standards, such as water quality standards and cleanup target levels; and
· imports the latest monitoring data into the Department’s Water Assurance Compliance
System (WACS) database via public file transfer protocol (ftp).
The Division of Waste Management maintains a ‘library’ within ADaPT of analytes and
associated laboratory methods.

The ADaPT Electronic Data Deliverable (EDD) consists of three electronic deliverables:
· a Laboratory EDD, identified as "HWldd";
· a Laboratory EDD Error Log, identified as "HWldd_ErrorLog ";
· a Field EDD identified as "HWfdd."
The Laboratory EDD shall be submitted in a comma separated (.csv format) text file which can be produced through Microsoft Excel. The Laboratory EDD file name format shall be: Florida Facility I.D. underscore Sampling Date (yyyymmdd) underscore HWldd. The period at the end would not be included. For example, with Florida Facility I.D. FLD000012345 and where sampling started November, 28 and ended on December, 4 2008 the Laboratory EDD file name should be FLD000012345_20081204_HWldd.txt
The Field EDD shall be submitted in the same comma separated (.csv format) text file as the Laboratory EDD. The Field EDD file name format shall be: Florida Facility I.D. underscore Sampling Date (yyyymmdd) underscore hwfdd. Again the period at the end is not included. For example, with Florida Facility I.D. FLD000012345 and where sampling started November, 28 and ended on December, 4 2008, the file name should be FLD000012345_20081204_HWfdd.txt.

Water quality monitoring reports shall be signed and sealed by a Florida registered professional geologist or professional engineer with experience in hydrogeological investigations. A copy of the sealed signature page may be submitted electronically with the report provided that the seal is legible (gray the embossed seal and scan). Otherwise, you must submit an original sealed and signed page.
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In order to validate the quality assurance aspects of the laboratory EDD, the permittee shall ensure the laboratory processes the laboratory EDD through ADaPT using both their laboratory specific library and the Division of Waste Management library and correct or explain all noted errors prior to submittal. The appropriate entity (laboratory, consultant, or permittee) shall also process the hazardous waste field EDD through ADaPT using the DEP Division of Waste Management library and correct or explain all noted errors prior to submittal. As a final completeness check, the permittee or consultant shall process both the lab EDD and field EDD through ADaPT and confirm a successful export to disk prior to submitting the lab EDD, ADaPT EDD Error Log, field EDD and ADaPT EDD export file ADaPTHWYYYYMMDD.csv to the DEP.
Note that transferring the electronic data from ADaPT to the WACS database requires that each sampled well/location needs a corresponding WACS ID associated with it. The Department’s ADaPT webpage has up to date tables of this information for your ADaPT program. However, the WACS database generally contains only wells that are routinely monitored. Assessment wells and soils data, essentially one‐time samplings, are not included in the database at this time. Errors generated while using ADaPT that are based on a lack of WACS information should be noted but ignored in this situation.
Compliance with this direction will address the data submittal and quality assurance
requirements of Rule 62‐730.225(2) and (3) FAC.

The latest version of the ADaPT software in a zipped form is available for free at: https://www.floridadep.gov/waste/waste/content/adapt	and	ADaPT	training	is available from LDC and other consultants. It is the responsibility of those supplying data to the Department to use the latest version of ADaPT.
