4DIM VIEWER SETUP AND USE
Click on 4Dim_Setup.exe to install the viewer provided by C Tech Development Corporation.  

After the viewer has installed, you can open the model created for Kennedy Generating Station, KGS_3D_Creosote_Model.4d.

Click on the left mouse button to rotate the model.

Use the Current Frame arrows at the bottom of the image to move forward and back through the model views.

Use the mouse trackwheel to zoom in and out.

Use the right mouse button to move the model image within the frame.

