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	Florida Department of Environmental Protection (DEP)

Division of Water Resource Management

Bureau of Beaches and Coastal Systems

3900 Commonwealth Boulevard, Mail Station 300

Tallahassee, Florida 32399-3000

(850) 487-4475

	VIOLATION REPORT

	Inspection Date:
	Inspection Time:
	Permit File number (if applicable):
	City (if applicable):
	County:

	10-11-07
	2 pm
	BO-563
	Lauderdale-by-the-Sea
	Broward

	DEP Monument Number (distance and direction):
	Distance of activity seaward of control line:

	Approximately NO221’ / SO179’ of R-51, Broward County
	Approximately 200’ east of CCCL

	Property Owner’s Name:
	Address:
	Telephone Number:

	Pier Point Developers, LLC

“The Oriana” 
	Project Address:

4320 El Mar Drive, Lauderdale-by-the-Sea
	(561) 750-9970
(561) 620-0417

	Other Violator’s Name (if applicable):
	Address:
	Telephone Number:

	Seawood Builders/ A Division of Catalfumo, LLC
	565 E. Hillsboro Blvd., Deerfield Beach, FL  33441 
	(954) 421-4200

	Description of Alleged Violation:

	Placement of unclean sand-fill east of project site in the dune system

	Inspector’s Comments:

	I received an e-mail from Mr. Stephen Higgins of Broward County Environmental Protection Department, in response to correspondence from a citizen concerned about unclean sand-fill placed on the beach, east of current project site for “The Oriana”.  It was initially reported that the fill consists of “broken glass, concrete chunks (flat pieces and pieces of concrete curbstones with metal sticking out), pieces of rusty metal (nails, reinforcing steel, flat pieces with sharp edges, 15” pieces of rusty ¼” rod), broken ceramic tile, metal and wood fence posts that terminate close to the surface, and electrical cable that sticks up through the surface”. Since I did not excavate any material (more than 6”) during my site visit, I can not verify the depth or extent of debris/rubble existing beneath the surface of the fill material. The site had been partially cleaned since the initial report describing the amount of debris-type items existing in the fill.  Less debris existed upon my arrival than in photos that had been sent to me by David Stout of Broward County EPD, indicating what he had observed at the time of his visit.  I observed mostly small chunks of concrete rubble mixed in the fill, ranging from .25” to 1.25” in size, with a couple larger pieces in some areas 2”-3”. Recent landscape installation should be considered when contemplating Enforcement Action. (Removal of sand for screening/sifting, replacement of fill, etc.)

	Action Taken:

	I met with on site with Lilianne Smatt of Coastal Systems Intl. and Project Engineer @ SeaWood Builders, Matthew Nichols, to discuss the issue. For the present, the “Oriana” construction crew will be utilizing hand tools (rakes, plastic buckets, etc.) to remove any excess rubble that they can locate in the fill.  They will continue this process until time of project completion or until it is indicated that further actions are required to alleviate the problem.  Use of  a “Sand-Man” (walk-behind sand-sifter machine) to effectively remove rubble from the property is another option.
A Warning Notice has been issued.
(See Photos) 

	

	
	Inspector’s Signature:
	
	Date:
	

	
	Wesley Cich
	
	10-11-07
	

	

	FOR TALLAHASSEE OFFICE USE (Routing, Review, and Comments):

	


	Photographs (including brief location description):
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Looking north from southeast side of property                              looking north from SE property (Zoom)                     
Coconut Palms are east of original construction-fencing; farthest extent of fill material placement
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Looking south from northeast side of property                             View looking south from NE (Zoom)
Fence that remains indicates former construction-fence line (tied into NE and SE property lines); also rough extent of fill placement
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Largest pieces of rubble, still a working area                                more rubble/debris
[image: image7.jpg]


 [image: image8.jpg]



Many small pieces of concrete rubble; Shell also shown               evidence of concrete rubble pieces in landscaping
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Small concrete pieces at beach access entrance/exit                      random small pieces of concrete debris
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Small pieces scattered in landscaping                                            small concrete pieces  
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Some concrete rubble/debris has been exposed east of fill-placement zone (compare with tree line in photos above)
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Some larger pieces I gathered 
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