Comments of FSA
Draft Revisions to Volume 1, Section 2
ERP Applicants Handbook




[bookmark: _Hlk95213925]14. 	“Best Management Practice (BMP)” means the structural, vegetative, or managerial practices used to treat, prevent, or reduce water pollution. Erosion and sediment control BMPs are structural and often temporary. Stormwater BMPs treat, prevent or reduce the nutrient load and other pollutants in water, are permanent in nature, and can be structural or nonstructural. 

Comment:  Not all E&S BMPs are structural and/or temporary.  Not all Stormwater BMPs are permanent.



[bookmark: _Hlk95376675]29.	"Detention with filtration" or "Filtration" means the selective removal of pollutants from stormwater by the collection and temporary storage of stormwater and the subsequent gradual release of the stormwater into surface waters in the state through at least 2 feet of suitable fine textured granular media such as porous soil, uniformly graded sand, or other natural or artificial fine aggregate, which may be used in conjunction with filter fabric and/or perforated pipe.

Comment:  Sand filters do not remove nutrients.


[bookmark: _Hlk97707988]
29.	“Discharge” means to allow or cause water to flow.

Comment:  This term is used in Chapter 8, so why delete it?


56. 	“Hydrologic Unit Code” or “HUC” means the hydrologic cataloging unit assigned to a geographic area representing a surface watershed drainage basin. A complete list of Hydrologic Unit codes, descriptions, names, and drainage areas can be found in the United States Geological Survey Water-Supply Paper 2294, entitled "Hydrologic Unit Maps".

[bookmark: _Hlk105052522]Comment:  Is there a more recent or up-to-date document to reference?





73.	“Net improvement performance standard” means the minimum performance standard(s) for treating stormwater wherein the nutrient or other pollutant loads discharged from the existing land use of the project area are less than reduced from those discharged pollutant loads generated in the project area’s pre-development conditions. See Section 8 for Performance Standard(s) criteria. 

Comment:  Clarification.



86.	“Predevelopment nutrient loading” means the average annual nutrient loading based on the land use and activities of a site five years prior to the date the permit application is submitted. land cover that is legally in existence at the time of rule implementation (date). 

Comment:  The suggested revision brings the definition into consistency with the recommendations of the TAC.



93.	“Redevelopment” means the construction on sites having existing commercial, industrial, institutional, or residential land uses, excluding silviculture or agriculture, where all or part of the existing impervious surface will be replaced with the same or lesser intense land use as part of the proposed activity and has not been previously permitted. 

	Comment:  Are projects that replace existing uses with more intense land uses not considered redevelopment but are new development?


105.	“Seasonal high ground water table” (SHGWT) means the zone of saturated soil at the highest average elevation of the zone of saturated soil during the wettest season of the a typical year during periods of normal rainfall.

Comment:  Clarification.

